**1.Binary to grey code conversion**

1.Record the MSB most significant bit

2.Add the MSB to the next bit, record the sum and neglect the carry

3.Repeat the procedure